|  |
| --- |
| **STREET NAME PLATE SPECIFICATION E SOUTH NORTHAMPTONSHIRE - CONSERVATION AREAS** |
| **AUTHORITY** | **SOUTH NORTHAMPTONSHIRE COUNCIL**   |
| **Introduction statement:** | South Northamptonshire Council’s Building Control manages the specification, purchase and installation of new and replacement street name plates.South Northamptonshire Council order on average 20 name plates per year of this specification, although this is no guarantee of future requirements.South Northamptonshire Council anticipates placing orders for street nameplates in about 6 batches per year.  |
| **Plates:** | Manufactured from 11 Gauge Aluminium. Nameplates to be stove enamelled. Galvanised to BS EN ISO2009 and stove enamelled black. |
| **Plate depth:** | 150mm |
| **Lettering height:** | 100mm die pressed black letters  |
| **Lettering colour:** | Black |
| **Border size:** | 12.5mm raised border | **Border colour:** | Black |
| **Background colour:** | White non reflective | **Reverse colour:** | n/a |
| **Symbols:** | Where the new road is a cul-de-sac, with no other roads of a different name leading off it, the sign should be ordered with the traditional no through road ‘T’ symbol at the right hand end of the name plate (as diagram 816.1 of the Traffic Sign Regulations) in white and red on blue background. |
| **Crest:** |  None |
| **Installation on Stands** | Name plates on supports should be securely set in concrete so that the top of the plate is approximately 1 metre above ground level. |
| **Fixing to Walls and other Structures** | Where at the Council’s request walls or other structures are to be used to fix the name plate to, the same specification as above should be used without a back plate and the name plate securely screwed direct to the wall using “pozidrive” security screws.  |
| **Cappings:** | Welded caps |
| **Supports:** | Angle Frame welded to two 1350mm x 50mm x 50mm box section uprights with welded caps. |
| **Support Finish** | None | **Support Colour** | black |
| **Installation:** | Installation is required by nameplate supplier |
| **Delivery Time:** | See Specification A |
| **Delivery address:** | Delivery to site where nameplates required |
| **Additional Information** | Signs are to be sited so that they can be readily seen from both directions of the approach road but they must not obstruct any visibility splay. When on supports they should be sited in land which is to be adopted as public highway, tight to the back-edging kerb of the footpath or demarcation line.  |

Example of: **South Northamptonshire Specification E type:** Name Plate

