**Appendix 5**

**SCHEDULE OF RATES FOR NEW WORKS**

|  |  |  |
| --- | --- | --- |
| **Description of Work Required** | **If equivalent please state make & model** | **Price** |
| **Installation of External Cameras**   * Price to include camera & labour |  |  |
| External installation of Hikvision X (or equivalent).  Single installation. |  |  |
| External installation of Hikvision X (or equivalent).  Installation of 2 to 5 cameras. |  |  |
| External installation of Hikvision X (or equivalent).  Installation of 6 to 10 cameras. |  |  |
| External installation of Hikvision X (or equivalent).  Installation of 11 to 20 cameras. |  |  |
|  |  |  |
| External installation of Hikvision Bullet (or equivalent).  Single installation |  |  |
| External installation of Hikvision Bullet (or equivalent).  Installation of 2 to 5 cameras |  |  |
| External installation of Hikvision Bullet (or equivalent).  Installation of 6 to 10 cameras |  |  |
| External installation of Hikvision Bullet (or equivalent).  Installation of 10 to 20 cameras |  |  |
|  |  |  |
| **Installation of Internal Cameras**   * Price to include camera & labour |  |  |
| Internal installation of Hikvision Minidome (or equivalent).  Single installation. |  |  |
| Internal installation of Hikvision Minidome (or equivalent).  Installation of 2 to 5 cameras. |  |  |
| Internal installation of Hikvision Minidome (or equivalent).  Installation of 6 to 10 cameras |  |  |
| Internal installation of Hikvision Minidome (or equivalent).  Installation of 11 to 20 cameras. |  |  |
|  |  |  |
| Internal installation of Hikvision Fisheye (or equivalent).  Single installation. |  |  |
| Internal installation of Hikvision Fisheye (or equivalent).  Installation of 2 to 5 cameras |  |  |
| Internal installation of Hikvision Fisheye (or equivalent).  Installation of 6 to 10 cameras |  |  |
| Internal installation of Hikvision Fisheye (or equivalent).  Installation of 11 to 20 cameras |  |  |
| . |  |  |
| **Cabling** |  |  |
| Lay cables within buildings (ceiling voids, risers, underfloor space) up to 50 metres long |  |  |
| Lay cables within buildings (ceiling voids, risers, underfloor space) 50 to 100 metres long |  |  |
| Install camera cables in pole up to 15 metres high |  |  |
| Lay camera cables in duct up to 10 metres long |  |  |
| Lay camera cables in duct up to 50 metres long |  |  |
| Soft dig to lay duct – per metre |  |  |
| Hard dig to lay duct – per metre |  |  |
| Lay cables in equipment racks up to 10 metres long |  |  |
| Lay cables in equipment racks up to 10 to 50 metres long |  |  |
| Lay cables in equipment racks up to 50 to 100 metres long |  |  |
|  |  |  |
| **Deployable Camera Work**   * Prices shall include collecting & transporting all camera equipment; accessing/re-aligning/re-positioning aerials on roof as necessary; fixing camera to a pole; connecting video cable to control room. * The tender sum shall also include the provision of the appropriate maintenance manuals, service documentation and appropriate training for operation and maintenance staff. * The Contractor's price shall include for all hoists, scaffolding, barriers, signage, lighting and the like to enable him to properly and safely carry out the maintenance works. The tender submission should give details of the hoist vehicle that is proposed to be used for this contract. * The Contractor must provide for the efficient protection of the public in order to prevent mishaps and accidents whilst carrying out the duties herein and as part of his tender submission provide relevant health and safety method statements relating to this requirement * If this type of contract is let, it will be based on one man one vehicle working. Payment for more than one man or more than one vehicle will not be made except under exceptional circumstances. The Contractor shall state such circumstances in the form of tender * The Contractor’s labour rates shall be inclusive of an appropriate vehicle i.e. van or mobile hydraulic platform, irrespective of the type of vehicle |  |  |
| Install test & commission camera & control case for local operation.  Please quote hourly rate. |  |  |
| Install test & commission camera & aerials/transmitters for CCTV control room operation. Please quote hourly rate. |  |  |
|  |  |  |
| **Recorders** |  |  |
| Hikvision 9000 series I8 with separate POE |  |  |
| Hikvision 9000 series I16 with separate POE |  |  |
|  |  |  |
| **Day rate (8 hours) for any works not included in the above** |  |  |
|  |  |  |