**DRAFT SPECIFICATION**

*Please note this is a draft specification and subject to change.*

HPUK operates both the Port of Felixstowe and Harwich International Port

HPUK requires the provision of Tier 2 – Marine response counter pollution services as detailed within this specification.

The length of the service provision agreement will be for a total of three years.

Scope of Requirements

1. To fulfil the service requirements, the Contractor is required to be an MCA accredited Oil Spill Response Organisation as specified in 1998 OPRC Regulations.
2. The Contractor will be required to provide marine tier 2 pollution response on a rapid mobilisation 24/7, 365 days/year basis to a specified location within the Port of Felixstowe, Suffolk IP11 9LY and Harwich International Port Limited, Essex CO12 4SR for a three-year period.
3. In addition to rapid mobilisation 24/7, 365 days/years, the Contractor will be required to provide helpline/advice services to the HPUK sites.
4. The Contractor will be required to rapidly mobilise, respond, and provide technical assistance on site within 6 hours of receiving notification from either site.
5. The Contractor is to provide training and renewal of 2P and 5P certification for (32 x 2P; 32x 5P) persons at the locations specified in 1).
6. HPUK requires the Contractor to design, plan and execute a practical Incident Management Exercise (IME) to be conducted in Year 1 of the contract at one of the locations specified in paragraph 1.