**APPENDIX 1**

**SCHEDULE OF ATTENDANCES AND ASSOCIATED WORKS**

The Lift Sub-Contractor is to make due allowance within his tender for the following associated works and attendances:

| SCHEDULE OF ATTENDANCES AND ASSOCIATED WORKS |
| --- |
| Item | **ByLC** | **ByMC** | **N/A** | **Remarks** |
|  | Use of shared welfare facilities. |  |  |  |  |
|  | Space only for materials and plant. |  |  |  |  |
|  | Unloading. |  |  |  |  |
|  | Secure storage. |  |  |  |  |
|  | Distribution to proximity of works. |  |  |  |  |
|  | Site Safety lighting. |  |  |  |  |
|  | Three phase and single phase power supply for the lift. |  |  |  |  |
|  | Setting out. |  |  |  |  |
|  | Working drawings. |  |  |  |  |
|  | Comment on drawings. |  |  |  |  |
|  | Fire proofing to service holes passing through fire walls. |  |  |  |  |
|  | Special access / hard standing. |  |  |  |  |
|  | Hoisting / craneage. |  |  |  |  |
|  | Testing. |  |  |  |  |
|  | Power during testing and commissioning. |  |  |  |  |
|  | Protection of unfinished/completed works. |  |  |  |  |
|  | Provision of tools. |  |  |  |  |
|  | Competent full time supervisor. |  |  |  |  |
|  | Safety officer. |  |  |  |  |
|  | Protection of lift car. |  |  |  |  |
|  | Lifting beam installation and testing. |  |  |  |  |
|  | Lift Machine supporting steelwork. |  |  |  |  |
|  | Permanent shaft lighting and power. |  |  |  |  |
|  | Temporary task lighting/hand tools, leads etc. |  |  |  |  |
|  | Shaft scaffolding (when required). |  |  |  |  |
|  | Sealing of lift shaft interior walls. |  |  |  |  |
|  | Pit access ladder. |  |  |  |  |
|  | Guide fixings. |  |  |  |  |
|  | Entrance sills and architraves. |  |  |  |  |
|  | Entrance sill support angles. |  |  |  |  |
| In addition, the Lift Contractor (LC) shall place all waste arising from these works in the facility provided on site by the Main Contractor (MC). |