**C10/1001/2:**

**Site Inspection Photographs**

** **

**Image 1 and 2:** The existing bridge viewed first from Springfield Road, and then Burnside.

****

****

**Image 3 and 4:** Damage to the existing RSJ and handrails on the existing bridge

****

****

**Image 5 and 6:** Existing bridge viewed first from upstream direction, then downstream. Note the service duct running underneath the bridge.

****

****

**Image 7 and 8:** Existing brick abutments.

****

**Image 9:** Possible corrugated asbestos board formwork

****

**Image 10:** Surface water outfall below bridge.

****

**Image 11:** Service duct on the downstream side of the existing bridge.