QUOTATION REQUEST

Gosport Borough Council invite quotes from suppliers for the supply and delivery of landscaping and maintenance tools as detailed below for delivery between 22nd March 2021 and 2nd April 2021.

General considerations

The supplier must agree to Gosport Borough Council terms and conditions.

The tools listed are given as guideline to the nature of the tools required and the nature of the environment in which the materials are to be used.

Requirements

All products must conform to relevant BS:EN standards and be appropriate for use in a commercial grounds maintenance setting, therefore the emphasis is on a robust design that confers longevity onto the item.

Delivery is required week commencing March 22nd 2021 to;

Gosport Borough Council Countryside

Grange Farm

Little Woodham Lane

Gosport

Hants

PO13 8AB

It is desirable for the tools to be constructed from materials that are widely recyclable, or break down rapidly in the environment.

SPECIFICATION

Where possible the proposed tools should match the descriptions provided below, it is assumed that different manufacturers will offer a variation on the sizes given as a guide in the descriptions.

All cordless tools are to include a battery specific to the requirements of that item with a matching charging unit.

|  |  |  |  |
| --- | --- | --- | --- |
| **Required Number** | **Tool type and description** | **Bidder’s proposed make** | **Price (£)*****TOTAL price for the number of tools listed*** |
| 2 | 400mm Forged steel crowbar/utilitybar. |  |  |
| 1 | Tubular steel post rammer with reinforced top, two handles able to accommodate posts of at least 150 mm. |  |  |
| 1 | Ground breaking bar for starting post holes. |  |  |
| 1 | 10 lb Sledgehammer drop forged steel head, non-slip handle. |  |  |
| 1 | 6 or 7 lb Sledgehammer drop forged steel head, non slip handle. |  |  |
| 1 | Pick axe with hardened tempered steel head and 900mm handle |  |  |
| 1 | 5lb Mattock with tempered steel head and 900mm handle |  |  |
| 1 | 1 to 2 lb Micro pick and mattock |  |  |
| 1 | Scutch/brick hammer with forged steel head or carbon steel head. |  |  |
| 2 | 3 to 4 lb Lump hammer with forged steel or carbon steel head and 400mm handle. |  |  |
| 1 | 2 to 3 lb Axe with tempered steel or carbon steel head and 900mm handle |  |  |
| 1 | 1.5 to 2 lb Hatchet with tempered steel or carbon steel head and 400 mm handle |  |  |
| 1 | Pair of fold up sawhorses |  |  |
| 1 | Cordless Hammer Drill And Impact Driver Twin Pack. Similar to the Dewalt DCK266M2T 18V 2 X 4.0Ah XR. |  |  |
| 1 | Cordless oscilating quick change multitool with blades for a range of wood and other materials and case similar to the Dewalt DWE315KT-GB |  |  |
| 1 | Cordless sliding mitre saw |  |  |
| 1 | Cordless circular saw |  |  |
| 1 | Cordless jigsaw |  |  |
| 1 | Cordless angle grinder |  |  |
| 1 | Mixed screwdriver set similar to the Stanley 48 piece set with bag |  |  |
| 4 | Socket Set similar to the Magnussen1/4” drive socket set. |  |  |
| 2 | 48 piece imperial and metric spanner set. |  |  |
| 2 | Set of adjustable wrench in 3 sizes similar to the Bahco 3-90 set. |  |  |
| 1 | Pliers –Heavy Duty 4 x Combination4 x Long nose 1 x Side cutters1 x Adjustable1 x Wire cutting1 x Carpenters pincers1 x 12” Water pump pliers. |  |  |
| 1 | 3 Piece bolster and cold chisel set similar to the Roughneck guarded bolster set |  |  |
| 1 | Chisel set similar to the Stanley 5 piece bevel edge set. |  |  |
| 1 | 600 mm heavy duty bolt cutters |  |  |
| 1 | Hand Saws 1 x Rough 600 mm blade1 x Universal 355 mm blade1 x Hacksaw 300mm  |  |  |
| 1 | General builders trowel set |  |  |
| 1 | 1Stanley knife with retractable blade |  |  |
| 1 | General purpose scissors  |  |  |
| 4 | Hammers1 x Claw Hammer1 x Mallet  |  |  |
| 1 | Self-levelling rotary laser level with receiver and tripod |  |  |
| 1 | Spirit levels1 x General purpose 600mm1 x General purpose 1200 mm 1 x 240mm  |  |  |
| 1 | Tape Measures1 x 50m surveyors tape1 x 30 m surveyors tape1 x 10m heavy duty retractable tape1 x 5 m heavy duty retractable. |  |  |
| 1 | Torches1 x LED rechargeable flashlight minimum 100m beam distance.1 x Inspection Torch LED rechargeable |  |  |
| 1 | Tool For Tensioning Stainless Steel Sign Banding |  |  |

Total Value of tools proposed = £

QUOTATION PROCESS

Please return quotes through the South East Business Portal, also known as Proactis, this must be your full and final price.

Quotes are to be returned by 15th February 2021.

Evaluation

These works will be awarded on best value price, provided the quotation covers all of the required considerations detailed above.